국립환경과학원고시 제2017-54호

폐기물공정시험기준 개정

「환경분야 시험·검사 등에 관한 법률」제6조에 따른 「폐기물공정시험기준」(국립환경과학원고시 제2017-20호, 2017.8.11.)을 다음과 같이 일부 개정하여 고시합니다.

2017년 12월 12일

국 립 환 경 과 학 원 장

1. 개정부분

구분	번호	폐기물공정시험기준
개정	ES 06000.b	총칙 (Introduction)
	ES 06150.c	시료의 준비 (Sample Preparation)
	ES 06301.1c	강열감량 및 유기물 함량-중량법 (Loss on Ignition and Total Organics-Gravimetry)
	ES 06303.1a	수분 및 고형물-중량법 (Humidity and Total Solid-Gravimetry)
	ES 06403.1a	비소-수소화물생성-원자흡수분광광도법 (Arsenic-Hydride Generation-Atomic Absorption Spectrophotometry)
	ES 06403.2a	비소-유도결합플라스마-원자발광분광법 (Arsenic-Inductively Coupled Plasma-Atomic Emission Spectrometry)
	ES 06404.1a	수은-환원기화-원자흡수분광광도법 (Mercury-Cold Vapor-Atomic Absorption Spectrophotometry)
	ES 06701.1a	감염성미생물-아포균 검사법 (Infectious Microorganism - Spore-Forming Bacteria Test)
	ES 06701.2a	감염성미생물-세균배양 검사법 (Infectious Microorganism – Culture Test)
	ES 06701.3a	감염성미생물-멸균테이프 검사법 (Infectious Microorganism – Sterilization Indicator Tape Test)
신설	ES 06151.1	상향류 투수방식의 유출시험 (Up-flow Percolation Method)
	ES.06804.1	금수성-물과의 반응성 시험방법 (Test methods for substances which, in contact with water, emit flammable gases)
	ES.06805.1	산화성 시험방법-고상 (Test methods for oxidizing properties - solid)
	ES.06805.2	산화성 시험방법-액상, 반고상 (Test methods for oxidizing properties - liquid, semisolid phase)
	ES.06806.1	자연발화성-공기접촉에 의한 자연발화성 시험방법 (Test methods for pyrophoric properties)
	ES 06900.0	금속함량 (Metal-Contents)
	ES 06900.1	금속함량-원자흡수분광광도법 (Metal Contents-Atomic Absortion Spectrophotometry)
	ES 06900.2	금속함량-유도결합플라스마-원자발광분광법 (Metal Contents-Inductively Coupled Plasma-Atomic Emission Spectrometry)
	ES 06901.1	금속함량-비소-수소화물생성법-원자흡수분광광도법 (Metal Contents-Arsenic-Hydride Generation-Atomic Absortion Spectrophotometry)
	ES 06901.2	금속함량-비소-유도결합플라스마-원자발광분광법 (Metal Contents-Arsenic-Inductively Coupled Plasma-Atomic Emission Spectrometry)
	ES 06902.1	금속함량-카드뮴-원자흡수분광광도법 (Metal Contents-Cardmium-Atomic Absorption Spectrophotometry)
	ES 06902.2	금속함량-카드뮴-유도결합플라스마-원자발광분광법 (Metal Contents-Cardmium-Inductively Coupled Plasma-Atomic Emission Spectrometry)
	ES 06903.1	금속함량-납-원자흡수분광광도법 (Metal Contents-Lead-Atomic Absorption Spectrophotometry)
	ES 06903.2	금속함량-납-유도결합플라스마-원자발광분광법 (Metal Contents-Lead-Inductively Coupled Plasma-Atomic Emission Spectrometry)
	ES 06904.1	금속함량-구리-원자흡수분광광도법 (Metal Contents-Copper-Atomic Absorption Spectrophotometry)
	ES 06904.2	금속함량-구리-유도결합플라스마-원자발광분광법 (Metal Contents-Copper-Inductively Coupled Plasma-Atomic Emission Spectrometry)
	ES 06905.1	금속함량-크로뮴-원자흡수분광광도법 (Metal Contents-Chromium-Atomic Absorption Spectrophotometry)
	ES 06905.2	금속함량-크로뮴-유도결합플라스마-원자발광분광법 (Metal Contents-Chromium-Inductively Coupled Plasma-Atomic Emission Spectrometry)
	ES 06906.1	금속함량-수은-열적분해 아말감-원자흡수분광광도법 (Metal Contents-Mercury-Thermal Decomposition Amalgamation Atomic Absorption Spectrophotometry)

2. 세부 개정 내용의 확인

이 고시의 개정 전문은 법제처 「국가법령정보센터」“행정규칙”에서 확인하시기 바랍니다.(http://www.law.go.kr)

부칙

① (시행일) 이 고시는 고시한 날부터 시행한다.

② (재검토기한) 국립환경과학원장은 「훈령·예규 등의 발령 및 관리에 관한 규정」에 따라 이 고시에 대하여 2018년 1월 1일을 기준으로 매 3년이 되는 시점(매 3년째의 12월 31일까지를 말한다)마다 그 타당성을 검토하여 개선 등의 조치를 하여야 한다.